For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the left rear compartment side trim.
3. Disconnect the electrical connector from the pump.
4. Remove the cylinder hose (1,3) from the pump (5).
5. Use a shop towel in order to control hydraulic oil leakage.
6. Remove the pump nuts (6).
7. Remove the pump (5) with the motor.

### Installation Procedure

1. Install the pump (5) with the motor.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. in Cautions and Notices.

Install the pump nuts (6).

Tighten
Tighten the nuts to 6 N·m (53 lb in).

3. Install the cylinder hose (1, 3) to the pump (5).

Tighten
Tighten the cylinder hose fittings to 7 N·m (62 lb in).

4. Connect the electrical connector to the pump.
5. Install the left rear compartment side trim.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

6. Connect the negative battery cable.