For 1990-2009 cars

# MANIFOLD ABSOLUTE PRESSURE CORRECT CHART INFORMATION

#### VEHICLES AFFECTED: 1984 Camaro Models With 2.5L - L4 Engine

The subject chart shown on Page 6E2-75, Figure 69, of the bound 1984 Camaro Shop Manual (ST-368-84) is incorrect. Refer to Fig. 1, for correct chart C-1D.

Pleabe make a note of this change in your bound copy of the shop manual. The loose-leaf manual is correct.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.