For 1990-2009 cars

## Compressor Pressure Relief Valve Removal V5 - Conventional Mount

#### Tools Required

J 41790-A Compressor Holding Fixture

1. Install the compressor into the J 41790-A .
2. Remove the pressure relief valve (2) from the rear head of the compressor.

## Compressor Pressure Relief Valve Removal V7 - Direct Mount

#### Tools Required

J 41790-A A/C Compressor Holding Fixture

1. Remove the A/C compressor from the vehicle.
2. Clamp the J 41790-A in a vise and attach the A/C compressor to the J 41790-A .
3. Remove the pressure relief valve from the rear head of the A/C compressor.