For 1990-2009 cars

### Installation Procedure

1. Install the thrust selective washer on the input housing.
2. Install the stator shaft/selective washer o-ring assembly on the input housing.

The black race on the bearing goes toward the oil pump.

3. Install the reverse input clutch on the input clutch assembly.
4. Index the reverse input clutch plates with the input clutch hub. Make certain all clutch plates are fully engaged.
5. Install the reverse input and the input clutch assembly into the transmission case.
6. Index the 3rd and 4th clutch plates with the input internal gear.

• | Ensure that all clutch plates are fully engaged.

• | When properly assembled, the reverse input clutch housing will be located just below the case oil pump face.