For 1990-2009 cars

### Removal Procedure

Notice: The TP sensor is an electrical component. Do not soak the TP sensor in any liquid cleaner or solvent as damage may result.

1. Disconnect the TP sensor electrical connector.
2. Remove the TP sensor attaching screws.
3. Remove the TP sensor.

### Installation Procedure

1. Install the TP sensor on the throttle body with the throttle valve in the closed position. Make sure the TP sensor lever lines up with the TP sensor drive lever on the throttle shaft.
2. Install the TP sensor attaching screws.

Tighten
Tighten the TP sensor attaching screws to 2 N·m (18 lb in).

Refer to the

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
3. Connect the TP sensor electrical connector.