For 1990-2009 cars

# POWER STEERING RESERVOIR CAP SEEPAGE (REPLACE CAP)

#### Subject: POWER STEERING RESERVOIR CAP SEEPAGE (REPLACE CAP)

#### Models Affected: 1993 FIREBIRD MODELS WITH 3.4L ENGINE (RPO L32)

#### CONDITION:

--------- Some 1993 Firebird models with 3.4L V-6 engines (RPO L32), and assembled prior to VIN breakpoint P2211639 may exhibit a slight seepage of power steering fluid from between the pump reservoir and reservoir cap. This condition is apt to occur when the vehicle is operated in an aggressive manner and would appear as a slight wetting on the reservoir body.

#### CAUSE:

----- Power steering fluid slosh results in fluid migration past the cap seal and wetting of the reservoir body.

#### CORRECTION:

---------- Replace existing power steering pump reservoir cap with new cap, P/N 26009893.

#### PART AVAILABILITY:

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation: E8300

Use Applicable Labor Time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.