For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Support the transmission with a transmission jack.
3. Remove the transmission mount nut (2) and washer.
4. Remove the transmission support bolts (2).
5. Remove the transmission support (1).
6. Remove the transmission mount bolts.
7. Remove the transmission mount.

### Installation Procedure

1. Install the transmission mount.
2. Install the transmission mount bolts.

Tighten
Tighten the transmission mount bolts to 48 N·m (36 lb ft).

3. Install the transmission support (1).
4. Install the transmission support bolts (2).

Tighten
Tighten the transmission support bolts (2) to 57 N·m (43 lb ft).

5. Install the transmission mount nut (2) and washer.

Tighten
Tighten the transmission mount nut (2) to 105 N·m (77 lb ft).

6. Remove the transmission jack.
7. Lower the vehicle.