For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable.
2. Remove the fuel filler cap.
3. Raise the vehicle.
4. Disconnect the fuel tank vent valve hose (1).
5. Remove the fuel tank vent valve (2) from the rear brake hose bracket (3).

### Installation Procedure

1. Connect the fuel tank vent valve (2) to the fuel tank vent valve hose (1).
2. Install the fuel tank vent valve (2) to the rear brake hose bracket (3).
3. Lower the vehicle.
4. Install the fuel filler cap.
5. Connect the negative battery cable.