For 1990-2009 cars

### Removal Procedure

1. Remove the old molding from the door.
2. Mark the position of the molding with a length of masking tape.
3. Wash the area with soapy water and wipe dry.
4. Remove all traces of adhesive from the door using a oil-free naptha or alcohol.

### Installation Procedure

1. Remove the backing paper from the molding.
2. Measure 5.0-7.0 mm (0.2-0.28 in) from the front edge of the door (2) to the front edge of the molding.
3. Align the molding to the tape guideline and press firmly in place.