For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. On Camaro and Firebird vehicles, open the access door in the front bumper air deflector.
3. On Trans Am vehicles, remove the push pin retainers which are located at the bottom center of the front fascia.
4. Disconnect the electrical connector from the fog lamp.
5. Remove the fog lamp bulb from the electrical connector.

### Installation Procedure

1. Install the fog lamp bulb to the electrical connector.
2. Connect the electrical connector to the fog lamp.
3. On Trans Am vehicles, install the push pin retainers to the bottom center of the front fascia.
4. On Camaro and Firebird vehicles, close the access door in the front bumper air deflector.
5. Lower the vehicle.