For 1990-2009 cars

### Removal Procedure

1. Remove the brake rotor. Refer to Brake Rotor Replacement .
2. Rotate the parking brake adjusting nut until the adjuster is in closed (fully) seated position.
3. Remove the parking brake shoe assembly.

### Installation Procedure

1. Install the parking brake shoe assembly.
2. Adjust the parking brake shoe to drum clearance. Refer to Parking Brake Shoe Adjustment
3. Install the brake rotor. Refer to Brake Rotor Replacement .