For 1990-2009 cars

Application | Specification
--- | ---
Set | Check
Front Caster | 4.5 to 5.5 degrees | 4.0 to 6.0 degrees

- Cross Caster (Front)

-0.7 to 0.7 degrees

-0.7 to 0.7 degrees

Front Camber | -0.1 to 0.9 degrees | -0.6 to 1.4 degrees

- Cross Camber (Front)

-0.7 to 0.7 degrees

-0.7 to 0.7 degrees

- Individual Toe (Front)

-0.1 to 0.1 degrees

-0.1 to 0.1 degrees

- Total Toe (Front)

-0.2 to 0.2 degrees

-0.2 to 0.2 degrees

- Steering Wheel Angle (Front)

-3.5 to 3.5 degrees

-3.5 to 3.5 degrees

Rear Camber | -0.6 to 0.6 degrees | -0.6 to 0.6 degrees

- Cross Camber (Rear)

-0.6 to 0.6 degrees

-0.6 to 0.6 degrees

- Total Toe (Rear)

-0.3 to 0.3 degrees

-0.3 to 0.3 degrees

Rear Thrust Angle | -0.15 to 0.15 degrees | -0.15 to 0.15 degrees