For 1990-2009 cars

### Removal Procedure

1. Remove the I/P upper trim pad. Refer to Instrument Panel Upper Trim Pad Replacement in Instrument Panel, Gauges and Console.
2. Remove the DRL ambient light sensor (1) from the trim pad (2).

Twist the DRL ambient light sensor (1) counterclockwise.

3. Disconnect the DRL electrical connector (3) from sensor (1).

### Installation Procedure

1. Connect the sensor (1) to the DRL electrical connector (3).
2. Install the DRL ambient light sensor (1) to the trim panel (2).

Twist the DRL ambient light sensor (1) clockwise.

3. Install the IP upper trim pad. Refer to Instrument Panel Upper Trim Pad Replacement in Instrument Panel, Gauges and Console.