For 1990-2009 cars

#### Tools Required

J 41712 Oil Pressure Sensor Socket

Important: In order to completely drain the oil from the oil pan internal baffling, the bottom of the oil pan must be level during the oil drain procedure.

1. Remove the oil pan drain plug and allow the oil to drain.
2. Remove the engine oil filter.
3. Remove the right rear engine block coolant drain plug and allow the coolant to drain.
4. Remove the left front engine block coolant drain plug (if applicable) and allow the coolant to drain.
5. Remove the engine block coolant heater (if applicable) and allow the coolant to drain.
6. Use the J 41712 or equivalent in order to remove the oil pressure sensor (if required).