For 1990-2009 cars

### Removal Procedure

1. Remove the transmission oil pan and the filter. Refer to Automatic Transmission Fluid and Filter Replacement .
2. Remove the 1-2 accumulator. Refer to Accumulator Assembly .
3. Disconnect the internal wiring harness electrical connectors from the following components:

• | Transmission pressure switch (1)

• | 1-2 shift control solenoid (2)

• | 2-3 shift control solenoid (3)

• | Pressure control solenoid (4)

• | TCC PWM solenoid (5)

• | 3-2 control solenoid (6)

4. Remove the pressure control solenoid retainer.
5. Remove the pressure control solenoid.
6. Remove the 1-2 and 2-3 shift solenoid retainers.
7. Remove the 1-2 and 2-3 shift solenoids.
8. Remove the 3-2 control solenoid retainer.
9. Remove the 3-2 control solenoid.

### Installation Procedure

1. Install the 3-2 control solenoid.
2. Install the 3-2 control solenoid retainer.
3. Install the 1-2 and 2-3 shift solenoids.
4. Install the 1-2 and 2-3 shift solenoid retainers.
5. Install the pressure control solenoid.

Ensure that the electrical tabs are facing outboard.

6. Install the pressure control solenoid retainer and retaining bolts.

Tighten
Tighten the pressure control solenoid retaining bolt to 11 N·m (97 lb in).

7. Connect the internal wiring harness electrical connectors to the following components:

• | Transmission pressure switch (1)

• | 1-2 shift control solenoid (2)

• | 2-3 shift control solenoid (3)

• | Pressure control solenoid (4)

• | TCC PWM solenoid (5)

• | 3-2 control solenoid (6)

8. Install the 1-2 accumulator. Refer to Accumulator Assembly .
9. Install the transmission oil pan and the filter. Refer to Automatic Transmission Fluid and Filter Replacement .