For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Exterior Lights System Check performed? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Connect a test light between C216 terminal K and ground.
2. Turn the hazard switch on.

Does the test light flash off and on?

--

Go to Step 3

Go to Step 4

3 | Replace the turn/hazard switch assembly. Refer to Hazard Warning Switch Replacement . Is the repair complete? | -- | Go to Step 9 | --
4 | Connect a test light between the hazard lamp flasher terminal B and ground. Does the test light flash off and on? | -- | Go to Step 5 | Go to Step 6
5 | Repair a poor connection or open in CKT 27. Is the repair complete? | -- | Go to Step 9 | --
6 | Connect a test light between the hazard lamp flasher terminal A and ground. Does the test light flash off and on? | -- | Go to Step 7 | Go to Step 8
7 | Replace the hazard lamp flasher. Refer to Hazard Lamp Flasher Replacement . Is the repair complete? | -- | Go to Step 9 | --
8 | Repair a poor connection or open in CKT 140. Is the repair complete? | -- | Go to Step 9 | --
9 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all repairs been made?

--

Go to Exterior Lights System Check

--