For 1990-2009 cars

### Removal Procedure

1. Disconnect the harness connector the EVAP canister purge valve.
2. Disconnect the EVAP purg pipe from the EVAP canister purge valve (2).
3. Remove the retaining bolt (1) from the EVAP canister purge valve.
4. Remove the EVAP canister purge valve (2).

### Installation Procedure

1. Position the EVAP canister purge valve (2) on the intake.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the retaining bolt (1) to the EVAP canister purge valve (2).

Tighten
Tighten the retaining bolt (1) to 10 N·m (89 lb in).

3. Connect the EVAP purge pipe to the EVAP canister purge valve.
4. Connect the harness connector to the EVAP canister purge valve.