For 1990-2009 cars

# 1981-1982 IDLE SPEED CONTROL ASSEMBLY REPAIR KIT

A revised gear and shaft was released for 1982 production idle speed control assemblies. Idle speed control assemblies with the new gear and shaft can be identified by a yellow dot on the housing near the shaft.

In order to provide these improvements for service assemblies, two service repair packages have been released to repair 1981 and 1982 idle speed control assemblies. Applications are as follows:

PART NUMBER APPLICATION ------ ------------ 17079749 For J2000 Series equipped with the 1.8L engine (VIN Code G)

17079750 All other engines

The repair kit contains a gear and shaft assembly, boot, grease, instruction sheet, and adjustment specifications.

The repair kit should only be used if the motor within the I.S.C. assembly runs, but the plunger does not extend or retract properly.

The repair kit will not correct conditions which cause the motor within the I.S.C. assembly not to run.

#### WARRANTY INFORMATION

Labor Operation T3097 Time Allowance .8 Hr.*

*Includes .5 for I.S.C. motor R&R.

Do not claim J6410 (.5 hr.) plus T3097 (.3 hr.).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.