For 1990-2009 cars

## Instrument Panel Insulator Replacement Left Side

### Removal Procedure

1. Remove the I/P retainers (2).
2. Unhook the flange on the I/P insulator (1) from the side kick panel.
3. Detach the tab on the I/P insulator (1) from the retainer on the I/P.
4. Remove the I/P insulator (1) from the I/P.

### Installation Procedure

1. Attach the tab on the insulator (1) to the I/P.
2. Hook the flange on the insulator (1) to the side kick panel.
3. Install the I/P insulator (1) to the I/P.
4. Install the I/P insulator retainer (2).

## Instrument Panel Insulator Replacement Right Side

### Removal Procedure

1. Remove the I/P retainer (2) from the boss on the heater and air conditioning module.
2. Remove the retainers (1) from the insulator (3).
3. Detach the forward flange on the insulator (3) from the boss on the HVAC module.
4. Unhook the flange on the insulator (3) from under the side kick panel.
5. Remove the insulator (3) from the I/P carrier.

### Installation Procedure

1. Hook the flange on the instrument panel I/P insulator (3) over the side kick panel.
2. Attach the forward flange on the insulator (3) to the boss on the HVAC module.
3. Install the insulator (3) to the I/P carrier.
4. Install the retainer (1) to the insulator (3).
5. Install the retainer (2) to the boss on the HVAC module.