For 1990-2009 cars

## Ignition Coil Module Replacement 3.8L

### Removal Procedure

1. Remove the ignition coil and ignition control module. Refer to Ignition Coil and Ignition Coil Module Replacement .
2. Lay the module with coils on a clean work surface.
3. Remove the ignition coil bolts (2) from all the coils (1).
4. Remove the ignition coils (1) from the module (4).
5. Remove the ignition coil seals (3).
6. Remove the module (4) from the module bracket (5).

### Installation Procedure

1. Install the module (4) to the module bracket (5).
2. Install the ignition coil seals (3).
3. Install the ignition coils (1) to the module (4).
4. Install the ignition coil bolts (2).

Tighten
Tighten the ignition coil bolts (2) to 4 N·m (35 lb in).

5. Install the ignition coil and ignition control module. Refer to Ignition Coil and Ignition Coil Module Replacement .