For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Brakes

- Discard Thickness (See Important)

30.7 mm

1.209 in

- Maximum Lateral Runout

0.13 mm

0.005 in

- Minimum Thickness After Refinish

31.08 mm

1.223 in

- Minimum Wear Thickness

31.08 mm

1.223 in

- Rotor Thickness (New)

32 mm

1.26 in

Thickness Variation | 0.013 mm | 0.0005 in
Rear Brakes

- Discard Thickness

24.51 mm

0.965 in

- Maximum Lateral Runout

0.15 mm

0.006 in

- Minimum Wear Thickness

24.89 mm

0.980 in

- Rotor Thickness (New)

25.90 mm

1.020 in

- Minimum Thickness After Refinish

24.89 mm

0.980 in

- Rear Axle Shaft Flange

0.05 mm

0.002 in

Thickness Variation | 0.013 mm | 0.0005 in
Important: All brake rotors have a discard dimension cast into the rotor. Replace any rotor that does not meet this specification. After refinishing the rotor, replace any rotor that does not meet the maximum or minimum thickness after refinish specifications.