For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Exterior Lights System Check performed? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 | Check for a poor connection or open at C216. Is C216 OK? | -- | Go to Step 3 | Go to Step 4
3 | Replace the turn/hazard switch assembly. Refer to Hazard Warning Switch Replacement . Is the repair complete? | -- | Go to Step 5 | --
4 | Repair a poor connection or open at C216. Is the repair complete? | -- | Go to Step 5 | --
5 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all repairs been made?

--

Go to Exterior Lights System Check

--