For 1990-2009 cars

### Purpose

The basic function of the air/fuel metering system is to control air/fuel delivery to the engine. The best air/fuel mixture to minimize exhaust emissions is 14.7 to 1, which allows the catalytic converter to operate most efficiently. Fuel is delivered to the engine by individual fuel injectors mounted in the intake manifold near each intake valve.

The main control sensor is the Heated Oxygen Sensor (HO2S), located in the exhaust manifold. The HO2S tells the Powertrain Control Module (PCM) how much oxygen is in the exhaust gas and the PCM changes the air/fuel ratio to the engine by controlling the fuel injector on time. Because of the constant measuring and adjusting of the air/fuel ratio, the fuel injection system is called a Closed Loop system.

### Modes of Operation

The PCM monitors voltages from several sensors to determine the engine's fuel needs. Fuel is delivered under one of several conditions called modes. All modes are controlled by the PCM and are described below.

### Starting Mode

When the ignition is first turned ON the PCM energizes the fuel pump relay for two seconds, allowing the fuel pump to build up pressure. The PCM then checks the Engine Coolant Temperature (ECT) sensor and the Throttle Position (TP) sensor. During cranking, the PCM checks the crankshaft position signal in order to determine the proper air/fuel ratio for starting.

The PCM controls the amount of fuel delivered in the starting mode by changing how long the fuel injectors are energized. This is done by pulsing the fuel injectors for very short times.

### Run Mode

The run mode has two conditions called Open Loop and Closed Loop.

When the engine is first started and engine speed is above 725 RPM, the system is in Open Loop operation. In Open Loop the PCM ignores the signal from the Heated Oxygen Sensor (HO2S), and calculates the air/fuel ratio based on inputs from the TP, ECT, and MAF sensors.

The system remains in Open Loop until the following conditions are met:

1. The HO2S has a varying voltage output showing that it is hot enough to operate properly (this depends on temperature).
2. The ECT has reached a specified temperature.
3. A specific amount of time has elapsed since starting the engine.

The specific values for the above conditions vary with different engines. When these conditions are met, the system enters Closed Loop operation. In Closed Loop the PCM changes fuel injector on-time based on the signal from the HO2S. This allows the air/fuel ratio to stay very close to 14.7:1.

### Acceleration Mode

The PCM provides extra fuel when it detects a rapid increase in throttle position and air flow.

### Deceleration Mode

The PCM reduces the amount of fuel injected when it detects a decrease in throttle position and air flow. When deceleration is very fast, the PCM may cut off fuel completely for short periods.

### Battery Voltage Correction Mode

When battery voltage is low, the PCM will compensate for the weak spark by:

• | Increasing the amount of fuel delivered.

• | Increasing the idle RPM.

• | Increasing ignition dwell time.

### Fuel Cut Off Mode

The PCM has the ability to shut OFF the fuel injectors completely or selectively when certain conditions are met. This fuel shut off mode allows the powertrain to protect itself from damage and also improve its driveability.

The PCM will disable the injectors under the following conditions.

• | Ignition OFF (prevents engine run-on).

• | Ignition ON but no ignition reference signal (prevents flooding or backfiring).

• | High engine speed (above red line).

• | High vehicle speed (above rated tire speed).

• | Extended high speed closed throttle coastdown (reduce emissions and increases engine braking).

#### Fuel RPM cut off ranges:

Important: These RPM cut off ranges may vary according to PCM calibration, axle ratio, tire size, and tire rating.

1. Park and Neutral - 4000 RPM
2. Reverse - 4000 RPM
3. Drive - 5950 RPM

### Catalytic Converter Protection Mode

The PCM constantly monitors engine operation and estimates conditions that could result in high catalytic converter temperatures. If the PCM determines the catalytic converter may overheat, it causes the system to return to; Open Loop; operation and enriches the fuel mixture.