For 1990-2009 cars

## Counter Gear Shaft Disassemble T56 Base Model

#### Tools Required

• | J 22912-O1 Split Plate

• | J 39473 Mainshaft Bearing Installer

• | J 39511 Split Plate

• | J 39547 Press Adapter

Important: Do not replace tapered bearings unless inspection shows bearing damage.

1. Remove the small tapered bearing, using the J 22912-O1 with the J 39473 and a hydraulic press.
2. Discard the small tapered bearing.
3. Remove the large tapered bearing, using the J 39511 , the J 39547 , and a hydraulic press.
4. Discard the large tapered bearing.