For 1990-2009 cars

Table 1: | Body Control Module (BCM) C1
Table 2: | Body Control Module (BCM) C2
Table 3: | Body Control Module (BCM) C3

#### Body Control Module (BCM) C1

Connector Part Information |

• | 1208-9527

• | 6 Way F Metri-Pack 280 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 694 | Driver door unlock
B | GRY | 295 | Lock all output
C | RED/BLK | 780 | Lock all input
D | ORN/BLK | 781 | Unlock all input
E | GRY/BLK | 1663 | Passenger door unlock
F | -- | -- | Not used

#### Body Control Module (BCM) C2

Connector Part Information |

• | 1206-4752

• | 6 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 650 | Ground
B | ORN | 40 | Battery positive voltage
C | DK BLU | 75 | Retained accessory power (RAP)
D | BRN | 4 | Accessory positive voltage
E | DK BLU/WHT | 149 | Courtesy lamps feed
F | RED | 102 | Battery positive voltage

#### Body Control Module (BCM) C3

Connector Part Information |

• | 1211-0207

• | 32 Way F Metri-Pack 100 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1 | BLK | 650 | Ground
C2 | PPL/WHT | 1074 | Ignition key resistor return
C3 | -- | -- | Not used
C4 | PPL/WHT | 237 | Fasten seat belt indicator control
C5 | DK GRN | 220 | Starter enable (V6 VIN K)
C6 | DK GRN/WHT | 817 | Vehicle speed input (Gulf States)
C7 | GRY | 157 | Interior lamps command input
C8 | BLU/WHT | 624 | Park lamps relay control (Domestic)
C8 | YEL | 1977 | Rear fog lamp relay control (Europe)
C9 | BLK | BLK | Horn relay control
C10 | -- | -- | Not used
C11 | YEL/BLK | 625 | Starter relay control
C12 | GRY | 728 | Security indicator lamp control
C13 | BLK/WHT | 238 | Seat belt switch signal
C14 | LT GRN | 80 | Ignition key signal
C15 | YEL/BLK | 68 | Low coolant indicator latching
C16 | -- | -- | Not used
D1 | WHT | 156 | Courtesy lamps return
D2 | LT BLU | 263 | Shock sensor tamper input
D3 | BLK/WHT | 1576 | Rear compartment lid release signal
D4 | BRN | 253 | Rear compartment lid release relay control
D5 | PNK | 39 | Ignition positive voltage
D6 | YEL | 49 | Program input
D7 | WHT/BLK | 1037 | Ignition key resistor feed
D8 | DK BLU | 229 | Fuel enable
D9 | LT BLU | 187 | Rear fog lamp request (Europe)
D10 | -- | -- | Not used
D11 | GRY/BLK | 745 | Driver door open input
D12 | BLK/WHT | 746 | Passenger door input
D13 | ORN/BLK | 737 | Rear compartment lid ajar input
D14 | LT GRN | 1828 | Shock sensor shock input (Domestic)
D14 | BLK | 650 | Ground (Europe)
D15 | BRN | 9 | Park lamps feed
D16 | -- | -- | Not used