For 1990-2009 cars

### Removal Procedure

1. Open the window panel.
2. Remove the rear compartment lift window inner panel cover. Refer to Upper Rear Trim Finish Panel Replacement .
3. Remove the nuts (2).
4. Remove the striker (3).

### Installation Procedure

1. Install the striker (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the nuts (2).

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Install the rear compartment lift window inner panel cover. Refer to Upper Rear Trim Finish Panel Replacement .
4. Inspect the window panel operation. Adjust as needed. Refer to Rear Compartment Lift Window Panel Adjustment .