For 1990-2009 cars

# CLUTCH CHATTER-2.5L 4 OR 5 SPEED MANUAL

SOME 1982-83 "F" SERIES EQUIPPED WITH THE 2.5L L4 ENGINE AND EITHER THE MUNCIE 4-SPEED OR BORG-WARNER 5-SPEED MANUAL TRANSMISSION MAY EXHIBIT AN OBJECTIONABLE DRIVELINE DISTURBANCE DUE TO CLUTCH CHATTER. THIS CHATTER ORIENTED CONDITION CAN BE CORRECTED BY PERFORMING THE PROCEDURES OUTLINED IN CHEVY BULLETIN 83-T-69 AND REPLACING THE CLUTCH DRIVEN PLATE (DISC) ASSEMBLY WITH THE APPROPRIATE DRIVEN PLATE ASSEMBLY (LISTED BELOW) MADE WITH A NON-ASBESTOS FACING MATERIAL: TRANSMISSION 4-SPEED 5-SPEED DRIVEN PLATE ASSEMBLY 14091380 15590120* *CONTAINS ANTI-RATTLE FEATURE ALSO

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.