For 1990-2009 cars

### Disassembly Procedure

1. Remove the steering column lock cylinder set. Refer to Steering Column Lock Cylinder Set - Disassemble - Off Vehicle .
2. Remove the column housing cover end cap (2).

Remove the cruise control connector (3) from the base plate (1) and disconnect.

3. Remove 3 pan head 6-lobed socket screws (1) from the lock housing cover and sleeve assembly.
4. Remove the lock housing cover and sleeve assembly (1).

Remove the column housing cover end base plate (3) and the dimmer switch rod actuator (4).

5. Remove the wire protector shield.
6. Remove the switch actuator pivot pin (2) from the pivot and pulse switch assembly (1).