For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 37096 Flywheel Holding Tool

1. If equipped with a manual transmission remove the clutch pressure plate and driven disc. Refer to Clutch Pressure Plate and Clutch Driven Plate in Clutch.
2. Remove the automatic transmission, if equipped. Refer to Transmission Replacement in automatic Transmission - 4L60-E.
3. Use the J 37096 to hold the flywheel to loosen the flywheel bolts.
4. If equipped with the manual transmission, remove the following components:

4.1. | Remove the flywheel bolts (1).

4.2. | Remove the flywheel (2).

5. If equipped with the automatic transmission, remove the following components:

5.1. | Remove the flywheel bolts (1).

5.2. | Remove the flywheel (2).

### Installation Procedure

#### Tools Required

• | J 36660-A Torque Angle Meter

• | J 37096 Flywheel Holding Tool

1. If equipped with the automatic transmission, install the following components:

1.1. | Install the flywheel (2).

1.2. | Install the flywheel bolts (1) finger tight.

2. If equipped with the manual transmission, install the following components:

2.1. | Install the flywheel (2).

2.2. | Install the flywheel bolts (1) finger tight.

3. Use the J 37096 to hold the flywheel when tightening the flywheel bolts.
4. Tighten the flywheel bolts.

Tighten
Tighten the flywheel bolts to 15 N·m (11 lb ft). Use the J 36660-A to torque the flywheel bolts an additional 50 degrees.

5. Install the automatic transmission, if equipped. Refer to Transmission Replacement in automatic Transmission - 4L60-E.
6. If equipped with a manual transmission install the clutch pressure plate and driven disc. Refer to Clutch Pressure Plate and Clutch Driven Plate in Clutch.