For 1990-2009 cars

#### Lack of Power, Sluggish or Spongy

Checks | Action
--- | ---
DEFINITION: Engine delivers less than expected power. Little or no increase in speed when the accelerator pedal is pushed down part way.
Preliminary Checks |

• | Refer to Important Preliminary Checks Before Starting in Symptoms .

• | Search for bulletins.

• | Inspect the PCM grounds for being clean, tight and in the proper locations. Refer to Engine Controls Schematics .

• | Remove the air filter element and inspect for dirt or for being restricted. Refer to Air Cleaner Element Replacement and replace as necessary.

Fuel System Checks |

• | Inspect both injector fuses for being open. An open injector fuse causes four ignition coils and four injectors not to operate. Replace the fuse. Inspect the ignition coil circuits and the injector circuits for an intermittent short to ground.

• | Test for incorrect fuel pressure. Refer to Fuel System Diagnosis .

• | Test for a restricted fuel filter. Refer to Fuel System Diagnosis .

• | Test for a contaminated fuel condition. Refer to Alcohol/Contaminants-in-Fuel Diagnosis .

• | Inspect items that cause an engine to run rich (long term fuel trim near -13%). For a rich condition, refer to DTC P0132 HO2S Circuit High Voltage Bank 1 Sensor 1 and DTC P0152 HO2S Circuit High Voltage Bank 2 Sensor 1 .

• | Inspect items that can cause an engine to run lean (long term fuel trim near 24%). For a Lean condition, refer to DTC P0131 HO2S Circuit Low Voltage Bank 1 Sensor 1 and DTC P0151 HO2S Circuit Low Voltage Bank 2 Sensor 1 .

Sensor/System | Use a scan tool in order to monitor the KS system for excessive spark retard activity. Refer to Knock Sensor (KS) System Description .
Ignition System |

• | Inspect both injector fuses for being open. An open injector fuse causes four ignition coils and four injectors not to operate. Replace the fuse. Inspect the ignition coil circuit and the injector circuits for an intermittent short to ground.

• | Wet down the secondary ignition system with water from a spray bottle. Wetting the secondary ignition system may help locate damaged or deteriorated components. Look/listen for arcing or misfiring as water is applied.

• | Test for proper ignition voltage output with spark tester J 26792 . Refer to Electronic Ignition (EI) System Diagnosis .

• | Remove the spark plugs and inspect for the following:

- | Correct heat range; refer to Spark Plug Usage in Engine Electrical.

- | Wet plugs

- | Cracks

- | Wear

- | Improper gap

- | Burned electrodes

- | Heavy deposits

Refer to Spark Plug Visual Diagnosis in Engine Electrical.

• | An improper spark plug gap causes a driveability condition. Gap the spark plugs using a wire gauge gap tool. Refer to Spark Plug Replacement in Engine Electrical.

• | Determine the cause of the fouling before replacing the spark plugs. If the spark plugs are gas fouled, refer to DTC P0172 Fuel Trim System Rich Bank 1 or DTC P0175 Fuel Trim System Rich Bank 2 . If the spark plugs are coolant or oil fouled, refer to Oil Consumption Diagnosis in Engine Mechanical-5.7L or Loss of Coolant in Engine Cooling.

• | Inspect for loose ignition coil grounds. Refer to Electronic Ignition (EI) System Diagnosis .

Engine Mechanical |

• | Ensure that the engine coolant temperature is not above 132°C (270°F). This condition causes the PCM to operate in Engine Coolant Over temperature-Fuel Disabled Mode. While in Engine Coolant Over temperature-Fuel Disabled Mode, the PCM turns fuel off to four cylinders at a time to keep engine temperatures from reaching damaging levels. The customer perceives Engine Coolant Over temperature-Fuel Disabled Mode as a lack of power, miss, or rough idle. If the engine operates in Engine Coolant Over temperature-Fuel Disabled Mode, refer to Engine Overheating in Engine Cooling.

• | Excessive oil in combustion chamber-Leaking valve seals. Refer to Oil Consumption Diagnosis in Engine Mechanical-5.7L.

• | Low cylinder compression. Refer to Engine Compression Test in Engine Mechanical-5.7L.

• | For incorrect basic engine parts. Inspect the following:

- | Camshaft

- | Cylinder heads

- | Pistons, etc.

Refer to Engine Mechanical-5.7L.

Additional Checks |

• | Inspect the exhaust system for possible restrictions. Inspect for the following:

- | Inspect the exhaust system for damaged or collapsed pipes. Refer to Restricted Exhaust in Engine Exhaust.

- | Inspect the exhaust manifold for a collapsed inner wall. Refer to Exhaust Manifold Cleaning and Inspection in Engine Mechanical-5.7L.

- | Inspect the mufflers for heat distress or possible internal failure. Refer to Internal Muffler Rattles/Loss of Power in Engine Exhaust.

- | Inspect for possible plugged Three-Way catalytic converters by comparing exhaust system back pressure on each side of engine. Test the back pressure by removing AIR check valves near exhaust manifolds or the Heated Oxygen sensors. Refer to Restricted Exhaust in Engine Exhaust.

• | Test the Transmission Torque Converter Clutch (TCC) operation. Refer to Functional Test in Automatic Transmission 4L60-E.