For 1990-2009 cars

#### Component Resistance Table

Component | Pass Thru Pins | Resistance at 20°C | Resistance at 100°C | Resistance to Ground (Case)
--- | --- | --- | --- | ---
1-2 Shift Solenoid Valve | A, E | 19-24 ohms | 24-31 ohms | Greater than 250 K ohms
2-3 Shift Solenoid Valve | B, E | 19-24 ohms | 24-31 ohms | Greater than 250 K ohms
TCC Solenoid Valve | T, E | 21-26 ohms | 26-33 ohms | Greater than 250 K ohms
TCC PWM Solenoid Valve | U, E | 10-11 ohms | 13-15 ohms | Greater than 250 K ohms
3-2 Shift Solenoid Valve Assy. | S, E | 20-24 ohms | 29-32 ohms | Greater than 250 K ohms
Pressure Control Solenoid Valve | C, D | 3-5 ohms | 4-7 ohms | Greater than 250 K ohms
Transmission Fluid Pressure (TFP) Manual Valve Position Switch | Refer to Transmission Fluid Pressure Manual Valve Position Switch Resistance Check .
*Transmission Fluid Temperature (TFT) Sensor | M, L | 3088-3942 ohms | 159.3-198.0 ohms | Greater than 10 M ohms
Vehicle Speed Sensor | A, B VSS CONN | 1470-2220 ohms | 1800-2820 ohms | Greater than 10 M ohms
*Important: The resistance of this device is necessarily temperature dependent and will therefore vary far more than any other device. Refer to the Transmission Fluid Temperature Sensor portion of Electronic Component Description .