For 1990-2009 cars

## Counter Gear Shaft Assemble Main Shaft

#### Tools Required

• | J 39438 Bearing Installer

• | J 5590 Press Tube

1. Install a new large tapered bearing, using the J 39438 , U-blocks and a hydraulic press.
2. Install a new small tapered bearing, using the J 5590 and a hydraulic press.

## Counter Gear Shaft Assemble Extension Shaft

#### Tools Required

• | J 5590 Press Tube

• | J 39473 Bearing Installer

1. Install a new small tapered bearing, using the J 39473 with V-blocks and a hydraulic press.
2. Do the following when installing the 5th/6th speed synchronizer assembly:

2.1. | Start the press operation.

2.2. | Stop pressing before the keys engage the blocking ring slots.

2.3. | Lift and rotate the 5th speed gear in order to engage the keys with the blocking ring.

2.4. | Continue pressing until the synchronizer is seated.

3. Install the following parts in order:

3.1. | The 5th speed drive gear caged needle bearing

3.2. | The 5th speed drive gear

3.3. | The 5th speed drive gear blocking ring

3.4. | The 5th/6th speed synchronizer assembly (The ID groove on the sleeve faces 5th speed gear.) Use the J 5590 and a hydraulic press

4. Install the 6th speed drive gear blocking ring.
5. Install a new 5th/6th speed synchronizer retainer ring.
6. Install the 6th speed drive gear bearing spacer.
7. Install the 6th speed drive gear caged needle bearing.
8. Install the 6th speed drive gear.
9. Install the 6th speed drive gear thrust washer.
10. Install the 5th/6th speed shift fork.