For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Suitably support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
2. Disconnect the vehicle speed sensor electrical connector.
3. Remove the vehicle speed sensor bolt.
4. Remove the vehicle speed sensor and the O-ring seal. Use a suitable container in order to catch any transmission fluid that may spill.

### Installation Procedure

1. Install the vehicle speed sensor with a new O-ring seal.
2. Install the vehicle speed sensor bolt.

Tighten
Tighten the speed sensor bolt to 11 N·m (97 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Connect the vehicle speed sensor electrical connector.
4. Lower the vehicle.
5. Check transmission fluid, add as required. Refer to Transmission Fluid Check .