For 1990-2009 cars

# LEFT SIDE I/P RATTLE - REMOVE HEADLAMP SWITCH & WRAP WIRES

#### SUBJECT: LEFT SIDE INSTRUMENT PANEL RATTLE (REMOVE HEADLAMP SWITCH AND WRAP WIRES)

#### VEHICLES AFFECTED: 1988-91 PONTIAC FIREBIRD 'F'

#### Condition:

---------- Left side instrument panel rattle

#### Cause:

------- Headlamp switch wiring hits instrument panel carrier.

#### Correction:

------------ Remove switch as outlined in Service Manual and wrap wires in foam tape such as 3M 06370 or equivalent.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.