For 1990-2009 cars

#### Tools Required

• | J 23327-1 Clutch Spring Compressor

• | J 25018-A Clutch Spring Compressor Adaptor

1. Remove the reverse input clutch retaining ring.
2. Remove all reverse input clutch plates.
3. Install the J 23327-1 .
4. Remove the reverse input clutch spring retainer ring.
5. Remove the reverse input clutch spring assembly.
6. Remove the reverse input clutch piston assembly.