For 1990-2009 cars

Application | Specification
--- | ---
Set | Check
Front Caster | 5.0±0.5 degrees | 5.0±1.0 degrees
Cross Caster (Front) | 0.0±0.7 degrees | 0.0±0.7 degrees
Front Camber | 0.4±0.5 degrees | 0.4±1.0 degrees
Cross Camber (Front) | 0.0±0.7 degrees | 0.0±0.7 degrees
Individual Toe (Front) | 0.0±0.1 degrees | 0.0±0.1 degrees
Total Toe (Front) | 0.0±0.2 degrees | 0.0±0.2 degrees
Steering Wheel Angle (Front) | 0.0±3.5 degrees | 0.0±3.5 degrees
Rear Camber | 0.0±0.6 degrees | 0.0±1.6 degrees
Cross Camber (Rear) | 0.0±0.6 degrees | 0.0±0.6 degrees
Total Toe (Rear) | 0.0±0.3 degrees | 0.0±0.3 degrees
Rear Thrust Angle | 0.0±0.15 degrees | 0.0±0.15 degrees