For 1990-2009 cars

## Rear Compartment Rear Center Trim Panel Carpet Replacement Coupe

### Removal Procedure

1. Remove rear compartment side trim panels. Refer to Cargo Area Side Trim Panel Replacement .
2. Remove rear compartment trim panel carpet retainer (push clip).
3. Remove rear compartment trim panel carpet (1) from vehicle body (2).

### Installation Procedure

Important: If retainer (push clip) is damaged, replace retainer.

1. Install rear compartment trim panel carpet (1) into vehicle body (2).
2. Insert rear compartment trim panel carpet retainer (push clip).
3. Install rear compartment side trim panels. Refer to Cargo Area Side Trim Panel Replacement .

## Rear Compartment Rear Center Trim Panel Carpet Replacement Convertible

### Removal Procedure

1. Remove rear compartment trim panel carpet retainer (push clips) (3).
2. Remove rear compartment trim panel carpet (1) and side trim (2 & 4) from vehicle body (2).

### Installation Procedure

1. Install rear compartment trim panel carpet (1) and side trim (2 & 4) into vehicle body (2).
2. Insert rear compartment trim panel carpet retainers (push clips) (3).

Important: If retainers (push clips) are damaged, replace as necessary.