For 1990-2009 cars

### Removal Procedure

1. Remove the left side instrument panel insulator. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connectors.
3. Remove the following components from the pedal with the bracket (1):

• | Cruise control release switch (2)

• | Stoplamp and TCC switch (3)

• | Cruise control clutch switch (4) or cruise control clutch anticipate switch (6)

### Installation Procedure

1. Install the following components to the pedal with the bracket (1):

• | Cruise control release switch (2)

• | Stoplamp and TCC switch (3)

• | Cruise control clutch switch (4) or cruise control clutch anticipate switch (6)

2. Connect the electrical connectors.
3. Install the left side instrument panel insulator. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.
4. Adjust the following components. Refer to Stop Lamp Switch Adjustment .

• | Cruise control release switch (2)

• | Stoplamp and TCC switch (3)

• | Cruise control clutch switch (4) or cruise control clutch anticipate switch (6)