For 1990-2009 cars

## Fuel Hose/Pipes Assembly Replacement Rear Pipes

### Removal Procedure

#### Tools Required

• | J 34730-1A Fuel Pressure Gauge

• | J 42960-1 Fuel Tank Drain Hose

• | J 42960-2 Fuel Flapper Door Holder

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Relieve the fuel system pressure. Refer to the Fuel Pressure Relief Procedure .
3. Drain the fuel tank. Refer to Fuel Tank Draining .
4. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
5. Clean all fuel and EVAP pipe and hose connections and the surrounding areas before disconnecting in order to avoid possible contamination of the fuel system.
6. Remove the fuel tank. Refer to Fuel Tank Replacement .
7. Remove the EVAP purge pipe (7) from the EVAP canister.
8. Remove the EVAP canister vent solenoid hose (5).
9. Remove the EVAP pipe to fill limiter vent valve pipe (3).
10. Remove the fuel feed pipe (4) and the fuel return pipe (2) from the fuel sender pipes.
11. Remove the fuel feed and return pipes from the fuel tank.
12. Cap the fuel and EVAP pipes in order to prevent possible fuel system contamination.

### Installation Procedure

1. Remove the caps from the fuel and EVAP pipes.
2. Connect the fuel feed pipe (4) and the fuel return pipe (2) to the fuel sender pipes.
3. Install the fuel feed and return pipes into the fuel tank clips.
4. Install the EVAP pipe to fill limiter vent valve pipe (3).
5. Install the EVAP canister vent solenoid hose (5).
6. Connect the EVAP purge pipe (7) to the EVAP canister.
7. Install the fuel tank. Refer to Fuel Tank Replacement .
8. Lower the vehicle.
9. Refill the fuel tank.
10. Connect the negative battery cable.
11. Tighten the fuel filler cap.
12. Inspect for leaks.

12.1. | Turn the ignition switch ON for 2 seconds.

12.2. | Turn the ignition switch OFF for 10 seconds.

12.3. | Turn the ignition switch ON.

12.4. | Inspect for fuel leaks.

13. Perform the idle learn procedure. Refer to PCM Idle Learn Procedure .