For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
AIR Check Valves | 23 | 17 | --
AIR Pipe To Intake Manifold | 24 | 18 | --
AIR Pipe To Left Side Exhaust Manifold | 34 | 25 | --
AIR Pipes To Right Side Exhaust Manifold | 24 | 18 | --
AIR Pump | 5.6 | -- | 50
Clean Air Cover Attaching Screws | 3.2 | -- | 28
Crankshaft Position (CKP) Sensor | 4-6 | -- | 35-53
Crossover Tube Retainer Attaching Screws | 5 | -- | 44
EGR Valve | 22 | 16 | --
EGR Vacuum Control Signal Solenoid Valve | 34 | 25 | --
Engine Coolant Temperature (ECT) Sensor | 23 | 17 | --
EVAP Canister Solenoid Valve | 5.8 | -- | 52
Fuel Filter Fitting | 30 | 22 | --
Fuel Pressure Regulator Attaching Screw | 10 | -- | 89
Fuel Rail Attaching Bolts | 10 | -- | 89
Fuel Sender Assembly Retaining Nuts | 6.5 | -- | 58
Fuel Tank Strap Attaching Bolts | 33 | 24 | --
Fuel Tube Bracket Attaching Screw | 5 | -- | 44
Heated Oxygen Sensor (HO2S) | 41 | 30 | --
IAC Valve Attaching Screws | 3 | -- | 27
IAC Valve/Coolant Cover Attaching Screws | 3.2 | -- | 28
Fuel Tube Bracket Attaching Screw | 5 | -- | 44
Knock Sensor (KS) | 19 | 14 | --
Manifold Absolute Pressure (MAP) Sensor | 6 | -- | 50
Powertrain Control Module (PCM) Connector End Bolts | 8 | -- | 70
Throttle Body Attaching Bolts | 25 | 18 | --
Throttle Position (TP) Sensor Attaching Screws | 2 | -- | 18