For 1990-2009 cars

Step | Action | Value | Yes | No
--- | --- | --- | --- | ---
DEFINITION: The transmission does not shift into one gear.
1 | Remove the transmission. Refer to Transmission Removal or to Transmission Removal . Check for worn or damaged gearshift components. Are the gearshift components OK? | -- | Go to Step 2 | Go to Step 3
2 | Disassemble the transmission. Refer to Transmission Disassemble or to Transmission Disassemble . Look for worn or damaged synchronizer assemblies. Replace all worn or damaged parts. | -- | -- | --
3 | Replace the worn or damaged gearshift components. Refer to Transmission Disassemble or to Transmission Disassemble . Will the transmission shift gears? | -- | System OK | Go to Step 2