For 1990-2009 cars

### Removal Procedure

1. Remove the I/P trim pad. Refer to Instrument Panel Upper Trim Pad Replacement .
2. Remove the I/P cluster bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
3. Remove the instrument cluster bolts (1).
4. Remove the instrument cluster (2).

Gently pull the cluster straight out to disconnect the electrical connector (3).

### Installation Procedure

1. Install the instrument cluster (2).
2. Install the instrument cluster bolts (1).

Tighten
Tighten the instrument cluster bolts (1) to 2.2 N·m (19 lb in) in sequence as shown.

3. Install the I/P cluster bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
4. Install the I/P trim pad. Refer to Instrument Panel Upper Trim Pad Replacement .