For 1990-2009 cars

## Radio Replacement Chevrolet

### Removal Procedure

1. Unsnap the instrument panel (IP) accessory trim plate (2).
2. Disconnect the electrical connectors (1) from the switches (3), if equipped.
3. Remove the radio bracket bolts (2).
4. Slide the radio (1) out from the IP.
5. Disconnect the following components from the radio (1):

• | The antenna cable (2)

• | The IP wiring harness connector (3)

6. Remove the radio from the vehicle.

### Installation Procedure

1. Install the radio (1) to the vehicle.
2. Connect the following components to the radio:

• | The antenna cable (2)

• | The IP wiring harness connector (3)

3. Slide the radio into the IP.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the radio bracket bolts (2).

Tighten
Tighten the radio bracket bolts (2) to 1.8 N·m (16 lb in).

5. Connect the electrical connector (1) to the switches (3), if equipped.
6. Install the IP accessory trim plate (2).
7. Disable the radio Theftlock® feature.

## Radio Replacement Pontiac

### Removal Procedure

1. Unsnap the instrument panel (IP) accessory trim plate.
2. Remove the radio bracket bolts (1).
3. Slide the radio (2) out from the IP.
4. Disconnect the following components from the radio (4):

• | The IP wiring harness connector (1)

• | The remote CD connector (2)

• | The antenna cable (3)

5. Remove the radio from the vehicle.

### Installation Procedure

1. Install the radio (4) to the vehicle.
2. Connect the following components to the radio:

• | The antenna cable (3)

• | The remote CD connector (2)

• | The IP wiring harness connector (1)

3. Slide the radio (2) into the IP.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the radio bracket bolts (1) in the following sequence:

4.1. | Lower left

4.2. | Upper right

4.3. | Upper left

Tighten
Tighten the radio bracket bolts to 1.8 N·m (16 lb in).

5. Install the IP accessory trim plate.
6. Disable the radio Theftlock® feature.