For 1990-2009 cars

1. Remove the key from the ignition switch.
2. Connect the passenger yellow 2-way connector located behind the IP compartment.
3. Install the Connector Position Assurance (CPA) to the passenger yellow 2-way connector located behind the IP compartment door.
4. Install the right instrument panel insulator. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.
5. Connect the driver yellow 2-way connector located at the base of the steering column.
6. Install the Connector Position Assurance (CPA) to the driver yellow 2-way connector located at the base of the steering column.
7. Install the left instrument panel insulator. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.
8. Install the AIR BAG fuse to the IP fuse block. Refer to Fuse Block Schematics in Wiring Systems.
9. Install the IP fuse block access door. Refer to Instrument Panel Fuse Block Access Door in Instrument Panel, Gauges and Console.
10. Staying well away from both air bags, turn the ignition switch to the RUN position.

10.1. | The AIR BAG warning lamp will flash seven times.

10.2. | The AIR BAG warning lamp will then turn OFF.

11. Perform the SIR Diagnostic System Check if the AIR BAG warning lamp does not operate as described.