For 1990-2009 cars

### Removal Procedure

1. Set the park brake, if equipped with a manual transmission
2. Place the ignition switch in the RUN position, if equipped with a automatic transmission.
3. Place the shift lever in the NEUTRAL position.
4. Remove the shift control knob. Refer to Floor Shift Control Knob Replacement in Automatic Transmissions.
5. Remove the shift lever knob from the shift lever.
6. Remove the console trim plate. Refer to Console Trim Plate Replacement .
7. Remove the floor console bolts (1).
8. Raise the park brake handle as far as possible.

If the park brake handle cannot be pulled up far enough to remove the console, perform the following:

• | Release the park brake handle

• | Hold the adjuster pawl disengaged

• | Then park brake handle can be pulled up further.

9. Disconnect the power outlet connector.
10. Remove the floor console (2) from the vehicle.

### Installation Procedure

1. Install the console (2) to the vehicle.
2. Connect the power outlet connector.
3. Release the park brake handle.
4. Install the floor console bolts (1).

Tighten
Tighten the floor console bolts (1) to 8 N·m (71 lb in).

5. Install the console trim plate. Refer to Console Trim Plate Replacement .
6. Install the shift lever knob to the shift lever.
7. Install the shift control knob. Refer to Floor Shift Control Knob Replacement in Automatic Transmissions.
8. Place the shift lever in the PARK position.
9. Place the ignition switch in the OFF position.