For 1990-2009 cars

# REVISED WHEEL NUT TORQUES SERVICE MANUAL REVISION

REVISED WHEEL NUT TORQUES-1982 CAMARO AND CHEVETTE MODELS THE WHEEL NUT TORQUES LISTED ON PAGE 3E-10 AND 3E-13 OF THE 1982 CAMARO (ST-368-82) AND CHEVETTE (ST-357-82) SHOP MANUALS, RESPECTIVELY , ARE INCORRECT. CAMARO TORQUES SHOULD BE: STEEL WHEELS 110 N.M (80 LB. FT.) CAST ALUMINUM WHEELS 140 N.M (100 LB. FT.) CHEVETTE TORQUES SHOULD BE: ALL MODELS 110 N.M (80 LB. FT.)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.