For 1990-2009 cars

#### Tools Required

• | J 21867 Pressure Gage

• | J 42907 Oil Pressure Testing Tool

1. With the vehicle on a level surface, run the vehicle for a few minutes. Allow adequate drain down time of 2-3 minutes and measure the oil level.
2. If required, add the recommended grade engine oil and fill the crankcase until the oil level measures full on the oil level indicator.
3. Run the engine briefly, 10-15 seconds, and verify low or no oil pressure on the vehicle gage or light.
4. Listen for a noisy valve train or a knocking noise.
5. Inspect for the following:

• | Oil diluted by water or glycol, anti-freeze

• | Foamy oil

6. Remove the oil filter and install the J 42907 .
7. Install J 21867 or equivalent to the J 42907 .
8. Run the engine and measure the engine oil pressure.
9. Compare the readings to Engine Mechanical Specifications .
10. If the engine oil pressure is below specifications, inspect the engine for one or more of the following:

• | Oil pump worn or dirty

• | Refer to Oil Pump Cleaning and Inspection .

• | Oil pump-to-engine block bolts loose

• | Refer to Oil Pump, Screen and Crankshaft Oil Deflector Installation .

• | Oil pump screen loose, plugged, or damaged

• | Oil pump screen O-ring seal missing or damaged

• | Malfunctioning oil pump pressure regulator valve

• | Excessive bearing clearance

• | Cracked, porous, or restricted oil galleries

• | Oil gallery plugs missing or incorrectly installed

• | Refer to Engine Block Plug Installation .

• | Broken valve lifters

• | Repair as necessary

11. If the oil pressure reading on the J 21867 or equivalent is within specifications, inspect for the following:

• | Plugged or incorrect oil filter and/or malfunctioning oil bypass valve

• | Malfunctioning oil pressure gage or sensor

• | Repair as necessary