For 1990-2009 cars

#### Tools Required

J 36660-A Torque Angle Meter

1. Install the new cylinder head gasket.
2. Install the gasket over the locating pins, with the yellow side of the tab on the outboard side facing up.
3. Install the cylinder head over the locating pins and the gasket.
4. Install the cylinder head bolt finger tight.

Tighten
Tighten the cylinder head bolts in sequence on the first pass to 30 N·m (22 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Use the J 36660-A in order to tighten the cylinder head bolts on the second pass.

Tighten

• | Tighten the short bolts (3, 4, 7, 8, 11, 12, 15, 16) 67 degrees.

• | Tighten the medium bolts (14, 17) 80 degrees.

• | Tighten the long bolts (1, 2, 5, 6, 9, 10, 13) 80 degrees.

6. Install the spark plugs.

Tighten
Tighten the spark plugs to 20 N·m (15 lb ft).

7. Install the engine coolant air bleed pipe and bolts. Use a backup wrench on the pipe fittings when you install the bolts.

Tighten
Tighten the bleed pipe bolts to 40 N·m (30 lb ft).