For 1990-2009 cars

### Removal Procedure

1. Remove roof lift window panels. Refer to Lift-Out Panel Replacement .
2. Remove roof panel longitudinal bow finish molding bolts/screws (1) from molding (2).
3. Remove longitudinal bow finish molding (2) from vehicle roof (3).

### Installation Procedure

1. Install longitudinal bow finish molding (2) to vehicle roof (3).
2. Install roof panel longitudinal bow finish molding bolts/screws (1) to molding (2).

Tighten
Tighten the bolts/screws as they are installed in positions 5, 3, and 4 to 1.7 N·m (15 lb in).

3. Install roof lift window panels. Refer to Lift-Out Panel Replacement .