For 1990-2009 cars

# FRONT DOOR GLASS RETAINER ASSY (NEW PARTS USAGE)

#### SUBJECT: FRONT DOOR GLASS RETAINER ASSEMBLIES (COMMONLY CALLED "DOOR GLASS PATCH")

#### VEHICLES AFFECTED: 1991 "F" CAR

1991 "F" style vehicles built after the following VIN breakpoints will use a new type front door glass retainer assembly.

Chevrolet NL104152 Pontiac NL202399

The new part combines the vertical weatherstrip and plastic panel (used on earlier styles) into a single component.

If service of these parts is required, it is recommended that the part be replaced with the type part it was built with.

#### Example

Past models prior to 1992 VIN breakpoints, use the early type multi piece retainer.

#### Models built after VIN breakpoints, use new components.

Part Numbers: 10198202 - Right ------------- 10198203 - Left

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.